# Capital-ship part placements — runtime-captured ground truth (see
# docs/re/ship-placement-runtime-capture.md and src/ship_capture.rs).
#
# Populate with:
#   SYLPHEED_ISO=... cargo run --release --example correlate_capture -- \
#     <capture.log> <Stage_SNN> <ship_id> [ref_part_substr] --emit
# then paste the emitted `ship …` block(s) below. The viewer prefers a ship's
# entry here over the static assembler when present.
#
# Per placement line: <part> <R00 R01 R02 R10 R11 R12 R20 R21 R22> <T0 T1 T2>
#

ship e106 ref=e106_bdy_04
  e106_bdy_01 1 0 0 0 1 0 0 0 1 -263.9948 -150.43242 1164.8667
# 2026-08-12: this rotation was diag(-1,1,1) - the X-flip `correlate` bakes in
# when a draw's buffer is the mirror of the decoded one. With distinct anchor
# assignment the twins now decode to their OWN buffers (the container carries
# both halves), so the mirror lives in the data and the placement is plain
# identity. Re-emitting from the capture agrees: `1 0 0 0 1 0 0 0 1 264.04343`.
  e106_bdy_02 1 0 0 0 1 0 0 0 1 264.0088 -150.41339 1164.8651
  e106_bdy_03 1 0 0 0 1 0 0 0 1 0.0029247368 -34.517372 1075.878
  e106_bdy_04 1 0 0 0 1 0 0 0 1 0 0 0
  e106_brg_01 1 0 0 0 1 0 0 0 1 -0.005471501 153.31795 -164.03748
  e106_eng_01 0.8659965 -0.50002277 0 0.4829627 0.83651507 0.25885975 -0.12941553 -0.22417325 0.96592265 131.2386 -133.06625 -132.06075
  e106_eng_02 1 0 0 0 1 0 0 0 1 0.0013684053 -49.088192 -139.47827
  e106_wep_02_01 1 0 0 0 1 0 0 0 1 0.000040663195 49.126797 1009.06744
